# std::mbrtoc8

From cppreference.com
< cpp‎ | string‎ | multibyte

Defined in header `<cuchar>` |  |
std::size_t mbrtoc8( char8_t* pc8, const char* s, std::size_t n, std::mbstate_t* ps ); |  | (since C++20)

Converts a narrow multibyte character to UTF-8 encoding.

If `s` is not a null pointer, inspects at most `n` bytes of the multibyte character string, beginning with the byte pointed to by `s` to determine the number of bytes necessary to complete the next multibyte character (including any shift sequences). If the function determines that the next multibyte character in `s` is complete and valid, converts it to UTF-8 and stores the first UTf-8 code unit in *pc8 (if `pc8` is not null).

If UTF-8 encoding of the multibyte character in `*s` consists of more than one UTF-8 code unit, then after the first call to this function, `*ps` is updated in such a way that the next call to `mbrtoc8` will write out the additional UTF-8 code units, without considering `*s`.

If `s` is a null pointer, the values of `n` and `pc8` are ignored and the call is equivalent to std::mbrtoc8(NULL, "", 1, ps).

If UTF-8 code unit produced is u8'\0', the conversion state *ps represents the initial shift state.

The multibyte encoding used by this function is specified by the currently active C locale.

### Parameters

pc8 | - | pointer to the location where the resulting UTF-8 code units will be written
s | - | pointer to the multibyte character string used as input
n | - | limit on the number of bytes in s that can be examined
ps | - | pointer to the conversion state object used when interpreting the multibyte string

### Return value

The first of the following that applies:

- ​0​ if the character converted from `s` (and stored in *pc8 if non-null) was the null character
- the number of bytes [1...n] of the multibyte character successfully converted from `s`
- -3 if the next UTF-8 code unit from a character whose encoding consists of multiple code units has now been written to *pc8. No bytes are processed from the input in this case.
- -2 if the next `n` bytes constitute an incomplete, but so far valid, multibyte character. Nothing is written to *pc8.
- -1 if encoding error occurs. Nothing is written to `*pc8`, the value EILSEQ is stored in errno and the value of *ps is unspecified.

### Example

| This section is incomplete Reason: no example

### See also

c8rtomb (C++20) | converts UTF-8 string to narrow multibyte encoding (function)

Retrieved from "https://en.cppreference.com/mwiki/index.php?title=cpp/string/multibyte/mbrtoc8&oldid=108100"