# std::chrono::tai_clock

From cppreference.com
< cpp‎ | chrono

Defined in header `<chrono>` |  |
class tai_clock; |  | (since C++20)

The clock `std::chrono::tai_clock` is a Clock that represents International Atomic Time (TAI). It measures time since 00:00:00, 1 January 1958, and is offset 10 seconds ahead of UTC at that date (i.e., its epoch, 1958-01-01 00:00:00 TAI, is 1957-12-31 23:59:50 UTC).

Leap seconds are not inserted into TAI. Thus, every time a leap second is inserted into UTC, UTC falls another second behind TAI. As of December 2017, UTC is 37 seconds behind TAI, reflecting the 10-second initial offset and the 27 leap seconds inserted between 1958 and 2017. Thus, 2018-01-01 00:00:00 UTC is equivalent to 2018-01-01 00:00:37 TAI.

`tai_clock` meets the Clock requirements. It does not meet the TrivialClock requirements unless the implementation can guarantee that `now()` does not throw an exception.

### Time point family

Defined in namespace `std::chrono` |  |
template<class Duration> using tai_time = std::chrono::time_point<std::chrono::tai_clock, Duration>; |  | (since C++20)
using tai_seconds = tai_time<std::chrono::seconds>; |  | (since C++20)

operator<< (std::chrono::tai_time) (C++20) | performs stream output on a tai_time (function template)
from_stream (std::chrono::tai_time) (C++20) | parses a tai_time from a stream according to the provided format (function template)
to_stream (std::chrono::tai_time) (C++20) | outputs a tai_time into a stream according to the provided format (function template)

### Member types

Member type | Definition
`rep` | signed arithmetic type representing the number of ticks in the clock's duration
`period` | a std::ratio type representing the tick period of the clock, in seconds
`duration` | std::chrono::duration<rep, period>, capable of representing negative durations
`time_point` | std::chrono::time_point<std::chrono::tai_clock>

### Member constants

constexpr bool is_steady [static] | true if the time between ticks is always constant, i.e. calls to `now()` return values that increase monotonically even in case of some external clock adjustment, otherwise false (public static member constant)

### Member functions

now [static] | returns a std::chrono::time_point representing the current point in time (public static member function)
to_utc [static] | converts `tai_time` to `utc_time` (public static member function)
from_utc [static] | converts `utc_time` to `tai_time` (public static member function)

Retrieved from "https://en.cppreference.com/mwiki/index.php?title=cpp/chrono/tai_clock&oldid=104740"